1.	Take apart the microphone and disconnect the blue wire.  
2.	Insulate the end with a piece of electrical tape and leave it loose.
3.	Connect the black wire to where the blue wire was connected. 
            I use mic gain set to 5 for working SSB with the ICOM 706.